**IOT BASED SAFETY GADGETS FOR CHILD SAFETY MONITORING AND NOTIFICATION**

**ASSIGNMENT**

void setup()

{

pinMode(LED\_BUILTIN, OUTPUT);

}

void loop()

{

digitalWrite(LED\_BUILTIN, HIGH);

delay(1000); // Wait for 1000 millisecond(s)

digitalWrite(LED\_BUILTIN, LOW);

delay(1000); // Wait for 1000 millisecond(s)

}

